Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Motion detector with 280° field of detection and large range
Special product features: One-hand plug-in base; Time-dependent operation modes, intelligent vandalism and sabotage protection, motion direction-dependent switch-off delay time, creep protection; Simple parameterisation, remote control and documentation with IR-Pen and App; Zero-cross switching; 
User interface: IR remote control
Control system: ON/OFF
Installation type: Surface mounting
Installation position: Ceiling / wall
Dimensions: Length 138 mm x Width 92 mm x Height/Depth 108 mm
Weight: 275 g
Protection type: IP55
Protection class: II
Impact resistance: IK07
Permissible ambient temperature: -25 °C...+50 °C
Relative humidity: 10 – 90%, non-condensing
Colour: white, similar to RAL 9003
Nominal voltage: 220 – 240 V AC / 50 – 60 Hz
In-rush current: 800 A / 200 µs
Detection angle: 280° (3 x 95° separately adjustable) and 360° creep protection
vertically tiltable by +90°/-10°
Detection range diagonally: Ø 40 m
Detection range head-on: Ø 10 m
Field of detection: up to 979 m²
Recommended installation height: 3 m
Max. mounting height: 6 m
Level of brightness: 2–2000 lx
Number of light channels: 1
Slave input: false
Constant light control: false
230 V/50 - 60 Hz
2300 W / 10 A (cos phi = 1),
1150 VA / 5 AX (cos phi = 0,5)
600 W LED
Switch contact: make contact / non-floating
Switch-off delay time: 60 s...240 min (adjustable in steps)
Impulse mode: true
Push button input: true